#	uugetty.sample: sample uugetty configuration file for a Hayes
#			compatible modem to allow incoming modem connections
#
# [ put this file in /etc/uugetty.<line> ]
#
# this config file sets up uugetty to use the RINGBACK feature for
# answering calls.

# ringback enable.  The defaults are trusted here (and are pretty sane).
# first, one to three rings, then hangup and call back within 6 and 60
# seconds.
RINGBACK=YES

MINRBTIME = 7
MAXRBTIME = 21
INTERRING = 6
MINRINGS = 1
MAXRINGS = 2

# line to use to do initialization.  All INIT, OFF, and WAITFOR functions
# are handled on this line.  If this line is not specified, any other
# program that wants to share the line (like kermit, uucp, seyon) will 
# fail.  This line will also be checked for lockfiles.
#
# format: <line> (without the /dev/)
INITLINE=cua3

# timeout to disconnect if idle...
TIMEOUT=60

# modem initialization string... Sets the modem not to auto-answer
#
# format: <expect> <send> ... (chat sequence)
INIT="" \d+++\dAT\r OK\r\n ATH0\r OK\r\n AT\sM0\sE1\sQ0\sV1\sX4\sS0=0\r OK\r\n

# waitfor string... if this sequence of characters is received over the line,
# a call is detected.
WAITFOR=RING

# this line is the connect chat sequence.  This chat sequence is performed
# after the WAITFOR string is found.  The \A character automatically sets
# the baudrate to the characters that are found, so if you get the message
# CONNECT 2400, the baud rate is set to 2400 baud.
#
# format: <expect> <send> ... (chat sequence)
CONNECT="" ATA\r CONNECT\s\A

# this line sets the time to delay before sending the login banner
DELAY=1
