# The getties in multi user mode on consoles an serial lines.
#
# NOTE NOTE NOTE adjust this to your getty or you will not be
#                able to login !!
#
# Note: for 'agetty' you use linespeed, line.
# for 'getty_ps' you use line, linespeed and also use 'gettydefs'
c1:1235:respawn:/sbin/getty tty1 VC linux
c2:1235:respawn:/sbin/getty tty2 VC linux
c3:1235:respawn:/sbin/getty tty3 VC linux
c4:1235:respawn:/sbin/getty tty4 VC linux
c5:1235:respawn:/sbin/getty tty5 VC linux
c6:1235:respawn:/sbin/getty tty6 VC linux
c7:1235:respawn:/sbin/getty tty7 VC linux
c8:1235:respawn:/sbin/getty tty8 VC linux
c9:1235:respawn:/sbin/getty tty9 VC linux
ca:1235:respawn:/sbin/getty tty10 VC linux
cb:1235:respawn:/sbin/getty tty11 VC linux
cc:12345:respawn:/sbin/getty tty12 VC linux

# Serial lines
s0:12345:respawn:/sbin/getty ttyS0 F19200 vt100
s1:12345:off:/sbin/getty ttyS1 F19200 vt100

# Dialup lines
#s0:12345:respawn:/sbin/uugetty ttyS0 M38400 dialup
#s1:12345:off:/sbin/uugetty ttyS1 M57600 dialup
s16:12345:respawn:/sbin/uugetty ttyS16 M57600 dialup
s17:12345:respawn:/sbin/uugetty ttyS17 M57600 dialup
s18:12345:respawn:/sbin/uugetty ttyS18 M57600 dialup
s19:12345:respawn:/sbin/uugetty ttyS19 M57600 dialup
s20:12345:respawn:/sbin/uugetty ttyS20 M57600 dialup
s21:12345:off:/sbin/uugetty ttyS21 M57600 dialup
s22:12345:off:/sbin/uugetty ttyS22 M57600 dialup
s23:12345:off:/sbin/uugetty ttyS23 M57600 dialup
